# Static Call Graph for image .\Debug\obj\mdk.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Thu Aug 29 16:09:48 2019

### Maximum Stack Usage = 96 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ EPD_partial_display ⇒ lut1 ⇒ EPD_W21_WriteDATA ⇒ SPI_Write

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- CAN1_RX1_IRQHandler ⇒ CAN1_RX1_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit_ExtMemCtl from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART4_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_hd.o(.text)
  - pic_display_4bit from main.o(.text) referenced from main.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000031))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 96 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ EPD_partial_display ⇒ lut1 ⇒ EPD_W21_WriteDATA ⇒ SPI_Write
  [Calls]
  - >> exit
  - >> main

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  GPIO_DeInit (Thumb, 172 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 274 bytes, Stack size 24 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> GPIO_Configuration

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> lcd_chkstatus

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> SPI_Write
  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD
  - >> EPD_W21_Init

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> SPI_Write
  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD
  - >> EPD_W21_Init

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 106 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EXTILineConfig (Thumb, 66 bytes, Stack size 12 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ETH_MediaInterfaceConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  RCC_DeInit (Thumb, 64 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_HSEConfig (Thumb, 70 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, stm32f10x_rcc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_GetFlagStatus
  [Called By]
  - >> RCC_Configuration
  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f10x_rcc.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCC_WaitForHSEStartUp ⇒ RCC_GetFlagStatus
  [Calls]
  - >> RCC_GetFlagStatus
  [Called By]
  - >> RCC_Configuration

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_PLLConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_SYSCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_HCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_PCLK1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_PCLK2Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration

  RCC_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 44 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_AHBPeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> RCC_Configuration
  - >> GPIO_Configuration

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  FLASH_SetLatency (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text))
  [Called By]

  - >> RCC_Configuration

  FLASH_HalfCycleAccessCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_PrefetchBufferCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text))
  [Called By]

  - >> RCC_Configuration

  FLASH_Unlock (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_Lock (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetStatus (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Called By]

  - >> FLASH_WaitForLastOperation

  FLASH_WaitForLastOperation (Thumb, 42 bytes, Stack size 16 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_GetStatus
  - >> delay
  [Called By]
  - >> FLASH_UserOptionByteConfig
  - >> FLASH_ReadOutProtection
  - >> FLASH_EnableWriteProtection
  - >> FLASH_ProgramOptionByteData
  - >> FLASH_ProgramHalfWord
  - >> FLASH_ProgramWord
  - >> FLASH_EraseOptionBytes
  - >> FLASH_EraseAllPages
  - >> FLASH_ErasePage

  FLASH_ErasePage (Thumb, 76 bytes, Stack size 16 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_EraseAllPages (Thumb, 72 bytes, Stack size 8 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_EraseOptionBytes (Thumb, 142 bytes, Stack size 8 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_ProgramWord (Thumb, 110 bytes, Stack size 24 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_ProgramHalfWord (Thumb, 64 bytes, Stack size 16 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_ProgramOptionByteData (Thumb, 72 bytes, Stack size 16 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_EnableWriteProtection (Thumb, 182 bytes, Stack size 32 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_ReadOutProtection (Thumb, 172 bytes, Stack size 16 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_UserOptionByteConfig (Thumb, 92 bytes, Stack size 24 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Calls]

  - >> FLASH_WaitForLastOperation

  FLASH_GetUserOptionByte (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetWriteProtectionOptionByte (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetReadOutProtectionStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetPrefetchBufferStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_GetFlagStatus (Thumb, 42 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  FLASH_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_flash.o(.text), UNUSED)

  SystemInit_ExtMemCtl (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(.text)

  Reset_Handler (Thumb, 14 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> CAN1_RX1_IRQHandler
  [Called By]
  - >> CAN1_RX1_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_hd.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  NMIException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  HardFaultException (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  MemManageException (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  BusFaultException (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  UsageFaultException (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  DebugMonitor (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  SVCHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  PendSVC (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  SysTickHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  WWDG_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN_TX_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  USB_LP_CAN_RX0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  CAN_RX1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  CAN_SCE_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text), UNUSED)

  EXTI9_5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  driver_delay_us (Thumb, 10 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> SPI_Write

  driver_delay_xms (Thumb, 26 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> EPD_W21_Init
  - >> EPD_full
  - >> EPD_partial_display
  - >> EPD_display_Clean
  - >> EPD_refresh
  - >> lcd_chkstatus

  DELAY_S (Thumb, 36 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = DELAY_S
  [Called By]
  - >> main

  lcd_chkstatus (Thumb, 42 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = lcd_chkstatus ⇒ EPD_W21_WriteCMD ⇒ SPI_Write
  [Calls]
  - >> EPD_W21_WriteCMD
  - >> driver_delay_xms
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> EPD_full
  - >> EPD_init_4Gray
  - >> EPD_partial_display
  - >> EPD_init
  - >> EPD_refresh
  - >> EPD_sleep

  EPD_sleep (Thumb, 38 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = EPD_sleep ⇒ lcd_chkstatus ⇒ EPD_W21_WriteCMD ⇒ SPI_Write
  [Calls]
  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD
  - >> lcd_chkstatus
  [Called By]
  - >> main

  EPD_refresh (Thumb, 20 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = EPD_refresh ⇒ lcd_chkstatus ⇒ EPD_W21_WriteCMD ⇒ SPI_Write
  [Calls]
  - >> EPD_W21_WriteCMD
  - >> lcd_chkstatus
  - >> driver_delay_xms
  [Called By]
  - >> main

  EPD_display_Clean (Thumb, 68 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = EPD_display_Clean ⇒ EPD_W21_WriteDATA ⇒ SPI_Write
  [Calls]
  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD
  - >> driver_delay_xms
  [Called By]
  - >> main

  EPD_init (Thumb, 120 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = EPD_init ⇒ lcd_chkstatus ⇒ EPD_W21_WriteCMD ⇒ SPI_Write
  [Calls]
  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD
  - >> EPD_W21_Init
  - >> lcd_chkstatus
  [Called By]
  - >> main

  lut1 (Thumb, 124 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = lut1 ⇒ EPD_W21_WriteDATA ⇒ SPI_Write
  [Calls]
  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD
  [Called By]
  - >> EPD_partial_display

  EPD_partial_display (Thumb, 284 bytes, Stack size 48 bytes, main.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = EPD_partial_display ⇒ lut1 ⇒ EPD_W21_WriteDATA ⇒ SPI_Write
  [Calls]
  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD
  - >> lut1
  - >> lcd_chkstatus
  - >> driver_delay_xms
  [Called By]
  - >> main

  EPD_init_4Gray (Thumb, 174 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = EPD_init_4Gray ⇒ lcd_chkstatus ⇒ EPD_W21_WriteCMD ⇒ SPI_Write
  [Calls]
  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD
  - >> EPD_W21_Init
  - >> lcd_chkstatus
  [Called By]
  - >> main

  pic_display_4bit (Thumb, 316 bytes, Stack size 24 bytes, main.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = pic_display_4bit ⇒ EPD_W21_WriteDATA ⇒ SPI_Write
  [Calls]
  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD
  [Address Reference Count : 1]
  - main.o(.text)

  lut11 (Thumb, 148 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = lut11 ⇒ EPD_W21_WriteDATA ⇒ SPI_Write
  [Calls]
  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD
  [Called By]
  - >> EPD_full

  EPD_full (Thumb, 28 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = EPD_full ⇒ lut11 ⇒ EPD_W21_WriteDATA ⇒ SPI_Write
  [Calls]
  - >> EPD_W21_WriteCMD
  - >> lut11
  - >> lcd_chkstatus
  - >> driver_delay_xms
  [Called By]
  - >> main

  PIC_display (Thumb, 60 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = PIC_display ⇒ EPD_W21_WriteDATA ⇒ SPI_Write
  [Calls]
  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD
  [Called By]
  - >> main

  GPIO_Configuration (Thumb, 140 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = GPIO_Configuration ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  RCC_Configuration (Thumb, 148 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = RCC_Configuration ⇒ RCC_WaitForHSEStartUp ⇒ RCC_GetFlagStatus
  [Calls]
  - >> FLASH_PrefetchBufferCmd
  - >> FLASH_SetLatency
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_PCLK2Config
  - >> RCC_PCLK1Config
  - >> RCC_HCLKConfig
  - >> RCC_GetSYSCLKSource
  - >> RCC_SYSCLKConfig
  - >> RCC_PLLCmd
  - >> RCC_PLLConfig
  - >> RCC_HSICmd
  - >> RCC_WaitForHSEStartUp
  - >> RCC_GetFlagStatus
  - >> RCC_HSEConfig
  - >> RCC_DeInit
  [Called By]
  - >> main

  main (Thumb, 782 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = main ⇒ EPD_partial_display ⇒ lut1 ⇒ EPD_W21_WriteDATA ⇒ SPI_Write
  [Calls]
  - >> RCC_Configuration
  - >> GPIO_Configuration
  - >> PIC_display
  - >> EPD_full
  - >> EPD_init_4Gray
  - >> EPD_partial_display
  - >> EPD_init
  - >> EPD_display_Clean
  - >> EPD_refresh
  - >> EPD_sleep
  - >> DELAY_S
  [Called By]
  - >> __rt_entry_main

  pic_4bit (Thumb, 164 bytes, Stack size 24 bytes, main.o(.text), UNUSED)
  [Calls]

  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD

  lut (Thumb, 124 bytes, Stack size 8 bytes, main.o(.text), UNUSED)
  [Calls]

  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD

  NVIC_Configuration (Thumb, 2 bytes, Stack size 0 bytes, main.o(.text), UNUSED)

  SPI_Delay (Thumb, 24 bytes, Stack size 0 bytes, display_epd_w21_spi.o(.text))
  [Called By]

  - >> SPI_Write
  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD

  SPI_Write (Thumb, 100 bytes, Stack size 16 bytes, display_epd_w21_spi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SPI_Write
  [Calls]
  - >> SPI_Delay
  - >> driver_delay_us
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> EPD_W21_WriteDATA
  - >> EPD_W21_WriteCMD

  EPD_W21_WriteCMD (Thumb, 48 bytes, Stack size 8 bytes, display_epd_w21_spi.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = EPD_W21_WriteCMD ⇒ SPI_Write
  [Calls]
  - >> SPI_Write
  - >> SPI_Delay
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> lut
  - >> pic_4bit
  - >> PIC_display
  - >> EPD_full
  - >> lut11
  - >> pic_display_4bit
  - >> EPD_init_4Gray
  - >> EPD_partial_display
  - >> lut1
  - >> EPD_init
  - >> EPD_display_Clean
  - >> EPD_refresh
  - >> EPD_sleep
  - >> lcd_chkstatus

  EPD_W21_WriteDATA (Thumb, 48 bytes, Stack size 8 bytes, display_epd_w21_spi.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = EPD_W21_WriteDATA ⇒ SPI_Write
  [Calls]
  - >> SPI_Write
  - >> SPI_Delay
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> lut
  - >> pic_4bit
  - >> PIC_display
  - >> lut11
  - >> pic_display_4bit
  - >> EPD_init_4Gray
  - >> EPD_partial_display
  - >> lut1
  - >> EPD_init
  - >> EPD_display_Clean
  - >> EPD_sleep

  EPD_W21_Init (Thumb, 50 bytes, Stack size 8 bytes, display_epd_w21.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = EPD_W21_Init
  [Calls]
  - >> driver_delay_xms
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> EPD_init_4Gray
  - >> EPD_init

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  ### Local Symbols

  delay (Thumb, 26 bytes, Stack size 8 bytes, stm32f10x_flash.o(.text), UNUSED)
  [Called By]

  - >> FLASH_WaitForLastOperation

  ### Undefined Global Symbols